LEDIL IES & EULUMDAT files


Please keep in mind that the files we provide are not 100% accurate.
We measure the lenses usually with 250mA current using symmetry when possible.
If the data you need is not available, please make a request.



